<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="50.526" y2="0" width="0.8128" layer="20"/>
<wire x1="50.526" y1="0" x2="50.526" y2="28.118" width="0.8128" layer="20"/>
<wire x1="50.526" y1="28.118" x2="0" y2="28.118" width="0.8128" layer="20"/>
<wire x1="0" y1="28.118" x2="0" y2="0" width="0.8128" layer="20"/>
<text>Fab FTDI</text>
<text>12 MHz</text>
<text>5V</text>
<text>3V</text>
</plain>
<libraries>
<library name="00fab">
<packages>
<package name="C1206FAB">
</package>
<package name="SOD123">
<description>&lt;b&gt;SMALL OUTLINE DIODE&lt;/b&gt;</description>
</package>
<package name="1X06SMD">
</package>
<package name="USB_MINIB">
</package>
<package name="SOIC16">
</package>
<package name="R1206FAB">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CRYSTAL-SMD-10.5X4.8-2PIN">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="00fab" package="C1206FAB" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="00fab" package="C1206FAB" value="10n"/>
<element name="C3" library="00fab" package="C1206FAB" value="22p"/>
<element name="C4" library="00fab" package="C1206FAB" value="22p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="00fab" package="SOD123" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="00fab" package="SOD123" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="00fab" package="1X06SMD" value="FTDI">
<attribute name="NAME"/>
</element>
<element name="U2" library="00fab" package="USB_MINIB" value="USB_MINIB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="00fab" package="SOIC16" value="CH340G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="SparkFun-FreqCtrl" package="CRYSTAL-SMD-10.5X4.8-2PIN" value="12MHz"/>
<element name="R1" library="00fab" package="R1206FAB" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U1" pad="8"/>
<contactref element="Y1" pad="P$1"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="Y1" pad="P$2"/>
<contactref element="C3" pad="2"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="GND">
<contactref element="U2" pad="GND"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="16"/>
<contactref element="J1" pad="3"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="D1" pad="CATHODE"/>
<contactref element="D2" pad="ANODE"/>
</signal>
<signal name="D-">
<contactref element="U2" pad="D-"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="D+">
<contactref element="U2" pad="D+"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="9"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="2"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="3"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$12">
<contactref element="U1" pad="14"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="3V3">
<contactref element="U1" pad="4"/>
<contactref element="D2" pad="CATHODE"/>
<contactref element="C2" pad="1"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="5V">
<contactref element="U2" pad="VBUS"/>
<contactref element="D1" pad="ANODE"/>
<contactref element="C1" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="GND'">
<contactref element="R1" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$3">
</signal>
</signals>
</board>
</drawing>
</eagle>
