<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="59.035" y2="0" width="0" layer="20"/>
<wire x1="59.035" y1="0" x2="59.035" y2="29.515" width="0" layer="20"/>
<wire x1="59.035" y1="29.515" x2="0" y2="29.515" width="0" layer="20"/>
<wire x1="0" y1="29.515" x2="0" y2="0" width="0" layer="20"/>
<text>CLK</text>
<text>Fab
FTDI</text>
</plain>
<libraries>
<library name="00fab">
<packages>
<package name="C1206FAB">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="2X03SMD">
</package>
<package name="1X06SMD">
</package>
<package name="R1206FAB">
</package>
<package name="USB_MINI">
</package>
<package name="TQFP32-08THIN">
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="HC49UP">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="00fab" package="C1206FAB" value="18p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="00fab" package="C1206FAB" value="18p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="00fab" package="C1206FAB" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="00fab" package="LED1206FAB" value="Red">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="00fab" package="2X03SMD" value="ISP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="00fab" package="1X06SMD" value="FTDI-SMD-HEADER">
<attribute name="NAME"/>
</element>
<element name="Q1" library="crystal" package="HC49UP" value="12MHz">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="00fab" package="R1206FAB" value="1k5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="00fab" package="R1206FAB" value="49">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="00fab" package="R1206FAB" value="49">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="00fab" package="R1206FAB" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="00fab" package="R1206FAB" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="00fab" package="USB_MINI" value="USB_MINI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="00fab" package="TQFP32-08THIN" value="ATmega8A-AU">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="00fab" package="R1206FAB" value="0"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="Q1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="N$2">
<contactref element="Q1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U2" pad="GND"/>
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="6"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="VCC">
<contactref element="D1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="J2" pad="3"/>
<contactref element="C3" pad="2"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="4"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U2" pad="VBUS"/>
<contactref element="D1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U2" pad="D-"/>
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U2" pad="D+"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R4" pad="2"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="N$14">
<contactref element="R5" pad="2"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="31"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="30"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="16"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="17"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="15"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$12">
<contactref element="J1" pad="5"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="D-">
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="D+">
<contactref element="R3" pad="2"/>
<contactref element="U1" pad="32"/>
</signal>
<signal name="N$13">
<contactref element="U1" pad="29"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$15">
</signal>
</signals>
</board>
</drawing>
</eagle>
