<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="62.21" y2="0" width="0" layer="20"/>
<wire x1="62.21" y1="0" x2="62.21" y2="35.23" width="0" layer="20"/>
<wire x1="62.21" y1="35.23" x2="0" y2="35.23" width="0" layer="20"/>
<wire x1="0" y1="35.23" x2="0" y2="0" width="0" layer="20"/>
<text>Fab FTDI</text>
<text>CLK</text>
</plain>
<libraries>
<library name="00fab">
<packages>
<package name="C1206FAB">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="2X03SMD-FAB">
<description>M2x03-SMD, wider pads</description>
</package>
<package name="1X06SMD">
</package>
<package name="R1206FAB">
</package>
<package name="USB_MINI">
</package>
</packages>
</library>
<library name="SparkFun-IC-Microcontroller">
<description>&lt;h3&gt;SparkFun Microcontrollers&lt;/h3&gt;
This library contains microcontrollers.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOP20W">
<description>&lt;b&gt;SMALL OUTLINE PACKAGE&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Clocks">
<description>&lt;h3&gt;SparkFun Clocks, Oscillators and Resonators&lt;/h3&gt;
This library contains the real-time clocks, oscillators, resonators, and crystals we use. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="HC49UP">
<description>&lt;h3&gt;HC-49/UP 11.4x4.8mm SMD Crystal&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://www.standardcrystalcorp.com/pdf%5Cc-3.pdf"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="00fab" package="C1206FAB" value="18p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="00fab" package="C1206FAB" value="18p"/>
<element name="C3" library="00fab" package="C1206FAB" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="00fab" package="LED1206FAB" value="Red">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="00fab" package="2X03SMD-FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="00fab" package="1X06SMD" value="FTDI-SMD-HEADER">
<attribute name="NAME"/>
</element>
<element name="R1" library="00fab" package="R1206FAB" value="49">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="00fab" package="R1206FAB" value="49">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="00fab" package="R1206FAB" value="1k5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="00fab" package="R1206FAB" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="00fab" package="R1206FAB" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="00fab" package="R1206FAB" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-IC-Microcontroller" package="SOP20W" value="ATTINY2313A">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-11305"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="00fab" package="USB_MINI" value="USB_MINI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="SparkFun-Clocks" package="HC49UP" value="12MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U2" pad="VBUS"/>
<contactref element="D1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="D1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="U1" pad="20"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="3"/>
<contactref element="C3" pad="2"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U2" pad="GND"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="10"/>
<contactref element="C3" pad="1"/>
<contactref element="JP1" pad="6"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="5"/>
<contactref element="Y1" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="Y1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="N$7">
<contactref element="R4" pad="1"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="N$8">
<contactref element="R5" pad="1"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="MOSI">
<contactref element="JP1" pad="4"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="MISO">
<contactref element="JP1" pad="1"/>
<contactref element="U1" pad="18"/>
</signal>
<signal name="SCK">
<contactref element="JP1" pad="3"/>
<contactref element="U1" pad="19"/>
</signal>
<signal name="RST">
<contactref element="JP1" pad="5"/>
<contactref element="U1" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="U2" pad="D-"/>
<contactref element="R1" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="U2" pad="D+"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="D-">
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="D+">
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="RXD">
<contactref element="U1" pad="2"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="TXD">
<contactref element="U1" pad="3"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$4">
</signal>
</signals>
</board>
</drawing>
</eagle>
